# 12.0 MACHINERY

## 12.1 Machinery Requirements

All machinery shall meet the following requirements:

* Operators Manual should be available onsite and referred to when new equipment is introduced to site
* Must have a clearly visible and operating emergency shut-off mechanism
* Must be in safe working condition and legally compliant
* Must be maintained according to manufacturer’s instructions
* Machinery requiring employees to work from unsafe heights must have slip resistant flooring, safety railing, and harnesses that can be attached

Machinery may include the following:

* Bench grinder
* Chassis machine
* Compressor
* Electric drill
* Grinder – hand held
* Inverta Spot GT
* Ladders
* Plasma cutter
* Pneumatic air tools
* Powered portable belt sanders
* Powered tools
* Sander / Polisher
* Spot welder
* Vehicle hoists
* Welding plant MIG
* Welding plant TIG
* Welding plant Gas